Example configuration

The LAN is considered DHCP powered and the TP-Link is OpenWRT powered. This configuration is for two tagged VLANs for two SSIDs

--- 8< --- /etc/config/network
...
config interface 'lan'
option ifname 'eth0'
option proto 'dhcp'
option hostname 'tp-link-coworkers'
config interface 'vlan101'
option type 'bridge'
option _orig_ifname 'eth0.101'
option _orig_bridge 'true'
option proto 'dhcp'
option ifname 'eth0.101'
config interface 'vlan102'
option type 'bridge'
option _orig_ifname 'eth0.102'
option _orig_bridge 'true'
option proto 'dhcp'
option ifname 'eth0.102'
...
--- >8 ---